* Software was developed for MRI using software-defined radios.
* It implements sequencing functionality, and calibrations and image reconstruction.
* It includes three common imaging sequences.
* It was validated in 0.5 Tesla MRI experiments.
* It enables the development of custom MRI spectrometers using off-the-shelf SDRs.